NSF/ANSI/CAN 61
Drinking Water System Components - Health Effects

NOTE: Unless otherwise indicated for Materials, Certification is only for the Water Contact Material shown in the Listing. Click here for a list of Abbreviations used in these Listings. Click here for the definitions of Water Contact Temperatures denoted in these Listings. Products certified to NSF/ANSI/CAN 61 comply with the health effects criteria in NSF/ANSI/CAN 600. 


 
	Clack Corporation 
	

	4462 Duraform Lane
	

	Windsor, WI 53598-9716
	
	 

	United States
	
	 

	608-846-3010
	
	




Facility : # 0 USA
Process Media

	 
	 
	Water
	Water

	 
	 
	Contact
	Contact

	Trade Designation
	Size
	Temp
	Material

	
Filtration Media[G] 

	Filter-Ag®
	10 x 34 mesh
	CLD 23
	SLDOX
	

	Filter-Ag®
	14 x 60 mesh
	CLD 23
	SLDOX
	

	
[G] Product is Certified to NSF/ANSI 372 and conforms with the lead content requirements for
    “lead free” plumbing as defined by California, Vermont, Maryland, and Louisiana state
    laws and the U.S. Safe Drinking Water Act.

    



NOTE: Certified for water treatment plant applications.
      This product has not been evaluated for point of use applications.


Facility : Windsor, WI
Mechanical Devices

	 
	 
	Water
	Water

	 
	 
	Contact
	Contact

	Trade Designation
	Size
	Temp
	Material

	
Miscellaneous Treatment Devices/Components [G] 

	1" & 1.25" Motorized Alternating Valve - V3069FF-01[1]
	.28 L
	CLD 23
	MLTPL
	

	1" & 1.25" Motorized Alternating Valve - V3069MM-01[1]
	.30 L
	CLD 23
	MLTPL
	

	1" & 1.25" No Hard Water Bypass Valve - V3070FF[1]
	.42 L
	CLD 23
	MLTPL
	

	1" & 1.25" No Hard Water Bypass Valve - V3070FM[1]
	.42 L
	CLD 23
	MLTPL
	

	1" Brass Sweat Assembly LF - V3007-02LF[1]
	.05 L
	CLD 23
	MLTPL
	

	1" Bypass Assembly - V3006[1]
	.13 L
	CLD 23
	MLTPL
	

	1" Bypass Assembly - V3006-XX[1] [11]
	.13 L
	CLD 23
	MLTPL
	

	1" John Guest QC Elbow Assembly - V3007-20[1]
	.04 L
	CLD 23
	MLTPL
	

	1" John Guest Straight QC Assembly - V3007-17[1]
	.1 L
	CLD 23
	MLTPL
	

	1" Meter Assembly - V3039[1]
	.11 L
	CLD 23
	MLTPL
	

	1" Meter Assembly - V3039-15[1]
	.11 L
	CLD 23
	MLTPL
	

	1" PVC Male BSPT Elbow Assembly - V3007-16[1]
	.08 L
	CLD 23
	MLTPL
	

	1" PVC Male NPT Elbow Assembly - V3007[1]
	.08 L
	CLD 23
	MLTPL
	

	1" Plastic Male BSPT Assembly - V3007-06[1]
	.05 L
	CLD 23
	MLTPL
	

	1" Plastic Male NPT Assembly - V3007-04[1]
	.05 L
	CLD 23
	MLTPL
	

	1" Sharkbite® Assembly - V3007-13LF[1]
	.08 L
	CLD 23
	MLTPL
	

	1" Twin Control Valve - TT1XX - VTT1AABCD-EFFGG[1] [2]
	2.06 L
	CLD 23
	MLTPL
	

	1'' Control Valve - WS1XX - V1AABCD-EFFGG[1] [2]
	.51 L
	CLD 23
	MLTPL
	

	1.25" Brass Sweat Assembly LF - V3007-09LF[1]
	.04 L
	CLD 23
	MLTPL
	

	1.25" Control Valve - WS125XX - V125AABCD-EFFGG[1] [2]
	.69 L
	CLD 23
	MLTPL
	

	1.25" PVC Solvent Assembly - V3007-07[1]
	.03 L
	CLD 23
	MLTPL
	

	1.25" Plastic Male BSPT Assembly - V3007-08[1]
	.08 L
	CLD 23
	MLTPL
	

	1.25" Plastic Male NPT Assembly - V3007-05[1]
	.08 L
	CLD 23
	MLTPL
	

	1.5" BSPT Meter - V3040BSPT[3]
	.25 L
	CLD 23
	MLTPL
	

	1.5" BSPT Meter - V3040BSPT-15[3]
	.25 L
	CLD 23
	MLTPL
	

	1.5" BSPT Motorized Alternating Valve (MAV) - V3071BSPT[3]
	.59 L
	CLD 23
	MLTPL
	

	1.5" BSPT No Hard Water Bypass Valve (NHWBP) - V3097BSPT[3]
	.52 L
	CLD 23
	MLTPL
	

	1.5" BYPASS ASSEMPLY - V4678[5]
	.53 L
	CLD 23
	MLTPL
	

	1.5" Brass Sweat Assembly LF - V3007-09LF[1]
	.08 L
	CLD 23
	MLTPL
	

	1.5" Control Valve - WS15XX - V15AABCD-EFFGG[3] [4]
	1.08 L
	CLD 23
	MLTPL
	

	1.5" NPT Meter - V3040[3]
	.25 L
	CLD 23
	MLTPL
	

	1.5" NPT Meter - V3040-15[3]
	.25 L
	CLD 23
	MLTPL
	

	1.5" NPT Motorized Alternating Valve (MAV) - V3071[3]
	.59 L
	CLD 23
	MLTPL
	

	1.5" NPT No Hard Water Bypass Valve (NHWBP) - V3097[3]
	.52 L
	CLD 23
	MLTPL
	

	1.5" PLASTIC FTG ASY QC TO BSPT SS - V4430-12[5]
	.09 L
	CLD 23
	MLTPL
	

	1.5" PLASTIC FTG ASY QC TO NPT SS - V4430-11[5]
	.09 L
	CLD 23
	MLTPL
	

	1.5" PVC Solvent Assembly - V3007-07[1]
	.08 L
	CLD 23
	MLTPL
	

	1.5" Plastic Control Valve - WS15P XX - VP15AABCD-EFFGG[4] [5]
	1.09 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC TO BSPT - V4430-02[5]
	.09 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC TO NPT - V4430-01[5]
	.09 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC TO QC - V4430-03[5]
	.09 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC to BSPT Elbow - V4430-08[5]
	.12 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC to NPT Elbow - V4430-07[5]
	.12 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC to QC Elbow - V4430-09[5]
	.14 L
	CLD 23
	MLTPL
	

	1.5" Plastic FTG ASY QC to Solvent - V4430-13[5]
	.14 L
	CLD 23
	MLTPL
	

	1.5" Plastic METER ASY BSPT 15FT - V3045BSPT-15[5]
	.13 L
	CLD 23
	MLTPL
	

	1.5" Plastic METER ASY BSPT 28IN - V3045BSPT[5]
	.13 L
	CLD 23
	MLTPL
	

	1.5" Plastic METER ASY NPT 15FT - V3045-15[5]
	.13 L
	CLD 23
	MLTPL
	

	1.5" Plastic METER ASY NPT 28IN - V3045[5]
	.13 L
	CLD 23
	MLTPL
	

	1.5" Plastic METER ASY QC TO QC 15FT - V3045QC-15[5]
	.13 L
	CLD 23
	MLTPL
	

	1.5" Plastic METER ASY QC TO QC 28IN - V3045QC[5]
	.13 L
	CLD 23
	MLTPL
	

	1.5" Plastic Motorized Alternating Valve (MAV) - V3034[5]
	.59 L
	CLD 23
	MLTPL
	

	1.5" Plastic No Hard Water Bypass Valve (NHWBP) - V3035[5]
	.54 L
	CLD 23
	MLTPL
	

	1.5" TWIN CONTROL VALVES - VT15AABCD-EFFGG[6]
	4.59 L
	CLD 23
	MLTPL
	

	1190FP In-Out Head w/ Fill Port - D1220-01[1]
	.48 L
	CLD 23
	MLTPL
	

	1191 In-Out Head - D1400[1]
	.35 L
	CLD 23
	MLTPL
	

	1191 In-Out Head w/ 1.320in Riser - D1400-03[1]
	.41 L
	CLD 23
	MLTPL
	

	1192 1.5 IN/OUT HEAD - D1403[1]
	.87 L
	CLD 23
	MLTPL
	

	1192 50MM IN/OUT HEAD - D1403-01[1]
	.87 L
	CLD 23
	MLTPL
	

	2" BSPT Meter - V3094BSPT[3]
	.37 L
	CLD 23
	MLTPL
	

	2" BSPT Meter - V3094BSPT-15[3]
	.37 L
	CLD 23
	MLTPL
	

	2" BSPT Motorized Alternating Valve (MAV) - V3076BSPT[3]
	.69 L
	CLD 23
	MLTPL
	

	2" BSPT No Hard Water Bypass Valve (NHWBP) - V3098BSPT[3]
	.63 L
	CLD 23
	MLTPL
	

	2" Control Valve - WS2XX - V2AABCD-EFFGG[3] [7]
	2.04 L
	CLD 23
	MLTPL
	

	2" HF Control Valve - WS2HF - V2HFABC-DD[8] [9]
	3.52 L 
	CLD 23
	MLTPL
	

	2" NPT Meter - V3094[3]
	.37 L
	CLD 23
	MLTPL
	

	2" NPT Meter - V3094-15[3]
	.37 L
	CLD 23
	MLTPL
	

	2" NPT Motorized Alternating Valve (MAV) - V3076[3]
	.69 L
	CLD 23
	MLTPL
	

	2" NPT No Hard Water Bypass Valve (NHWBP) - V3098[3]
	.63 L
	CLD 23
	MLTPL
	

	2" PLASTIC FTG ASY QC TO BSPT SS - V4460-12
	.19 L
	CLD 23
	MLTPL
	

	2" PLASTIC FTG ASY QC TO NPT SS - V4460-11
	.19 L
	CLD 23
	MLTPL
	

	2" Plastic Control Valve - WS2P XX - VP2AABCD-EFFGG[3] [7]
	2.12 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC TO BSPT - V4460-02[3]
	.19 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC TO NPT - V4460-01[3]
	.19 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC TO QC - V4460-03[3]
	.24 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC to BSPT Elbow - V4460-05[3]
	.32 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC to NPT Elbow - V4460-04[3]
	.32 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC to QC Elbow - V4460-06[3]
	.35 L
	CLD 23
	MLTPL
	

	2" Plastic FTG ASY QC to Solvent - V4460-13[3]
	.28 L
	CLD 23
	MLTPL
	

	2" Plastic METER ASY BSPT 15FT - V3048BSPT-15[3]
	.31 L
	CLD 23
	MLTPL
	

	2" Plastic METER ASY BSPT 28IN - V3048BSPT[3]
	.31 L
	CLD 23
	MLTPL
	

	2" Plastic METER ASY NPT 15FT - V3048-15[3]
	.31 L
	CLD 23
	MLTPL
	

	2" Plastic METER ASY NPT 28IN - V3048[3]
	.31 L
	CLD 23
	MLTPL
	

	2" Plastic METER ASY QC TO QC 15FT - V3048QC-15[3]
	.31 L
	CLD 23
	MLTPL
	

	2" Plastic METER ASY QC TO QC 28IN - V3048QC[3]
	.31 L
	CLD 23
	MLTPL
	

	2" Plastic Motorized Alternating Valve (MAV) - V3036[3]
	.99 L
	CLD 23
	MLTPL
	

	2" Plastic No Hard Water Bypass Valve (NHWBP) - V3037[3]
	.9 L
	CLD 23
	MLTPL
	

	2" Quick Connect Control Valve - WS2XX - V2AABCD-EFFGG[3] [4]
	2.04 L
	CLD 23
	MLTPL
	

	2” QC & 2H 4" BASE Assembly - V3064[3]
	.5 L
	CLD 23
	MLTPL
	

	2” QC & 2H 6" FLANGE BASE Assembly - V3055[3]
	1 L
	CLD 23
	MLTPL
	

	2” QC & 2H BSPT SIDE MOUNT Assembly - V3260BSPT-02[3]
	2.1 L
	CLD 23
	MLTPL
	

	2” QC & 2H NPT SIDE MOUNT Assembly - V3260-02[3]
	2.1 L
	CLD 23
	MLTPL
	

	3" BSPT Meter - V3095BSPT[3]
	1.64 L
	CLD 23
	MLTPL
	

	3" BSPT Meter - V3095BSPT-15[3]
	1.64 L
	CLD 23
	MLTPL
	

	3" BSPT Motorized Alternating Valve (MAV) - V3083BSPT[9]
	3.04 L
	CLD 23
	MLTPL
	

	3" BSPT No Hard Water Bypass Valve (NHWBP) - V3099BSPT[9]
	1.78 L
	CLD 23
	MLTPL
	

	3" BSPT Side Mount Base Assembly - V3674BSPT-02[3]
	1.03 L
	CLD 23
	MLTPL
	

	3" Control Valve - WS3 -V3ABC-DD[9] [10]
	5.59 L
	CLD 23
	MLTPL
	

	3" NPT Meter - V3095[3]
	1.64 L
	CLD 23
	MLTPL
	

	3" NPT Meter - V3095-15[3]
	1.64 L
	CLD 23
	MLTPL
	

	3" NPT Motorized Alternating Valve (MAV) - V3083[9]
	3.04 L
	CLD 23
	MLTPL
	

	3" NPT No Hard Water Bypass Valve (NHWBP) - V3099[9]
	1.78 L
	CLD 23
	MLTPL
	

	3" NPT Side Mount Base Assembly - V3674-02[3]
	1.03 L
	CLD 23
	MLTPL
	

	3/4" Brass Sweat Assembly LF - V3007-03LF[1]
	.01 L
	CLD 23
	MLTPL
	

	3/4" John Guest QC Elbow Assembly - V3007-15[1]
	.08 L
	CLD 23
	MLTPL
	

	3/4" John Guest QC Straight Assembly - V3007-19[1]
	.08 L
	CLD 23
	MLTPL
	

	3/4" Plastic Male BSPT Assembly - V3007-14[1]
	.04 L
	CLD 23
	MLTPL
	

	3/4" Plastic Male NPT Assembly - V3007-18[1]
	.04 L
	CLD 23
	MLTPL
	

	3/4" Sharkbite® Assembly - V3007-12LF[1]
	.05 L
	CLD 23
	MLTPL
	

	3/4" x 1" PVC Solvent Elbow Assembly - V3007-01[1]
	.08 L
	CLD 23
	MLTPL
	

	6" Flange Base Assembly - V3090[1]
	.66 L
	CLD 23
	MLTPL
	

	Air Blocker - D1047
	0 L
	CLD 23
	MLTPL
	

	DPMT-0948[1]
	0 L
	CLD 23
	MLTPL
	

	DPMT-0948-A[1]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1054[5]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1054-1320[5]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1054-32MM[5]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1054-A[5]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1252[3]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1252-1320[3]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1252-32MM[3]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1252-A[3]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1354[12]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1354-1320[12]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1354-32MM[12]
	0 L
	CLD 23
	MLTPL
	

	DPMT-1354-A[12]
	0 L
	CLD 23
	MLTPL
	

	External In-Line Mixing Valve - V4099[1]
	.1 L
	CLD 23
	MLTPL
	

	FITTING 2.5-8 - D1285[1]
	.11 L
	CLD 23
	MLTPL
	

	Inline Adapter Fitting - V3467[1]
	.13 L
	CLD 23
	MLTPL
	

	TOP DIFFUSER 1.050 WATER RIGHT - D1249WR[1]
	0 L
	CLD 23
	MLTPL
	

	Vertical Adapter Assembly - V3191-01[1]
	.26 L
	CLD 23
	MLTPL
	

	
[1] Certified for use with tanks 9 x 48 and greater.
[2] V1AABCD-EFFGG, VTT1AABCD-EFFGG, and V125AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be A, A2, A3, B, C, D, E, F, G, H, I, J, K, or Z to indicate the injector
    installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    in indicates colored covers or special labels on the cover.
[3] Certified for use with tanks 12 x 52 and greater.
[4] V15AABCD-EFFGG and VP15AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be B, C, D, E, F, G, H, I, or Z to indicate the injector installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    in indicates colored covers or special labels on the cover.
[5] Certified for use with tanks 10 x 54 and greater.
[6] Certified for use with tanks 14 x 65 and greater.
[7] V2AABCD-EFFGG and VP2AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be A, A2, A3, B, C, D, E, F, G, R, S, T, U, or Z to indicate the injector
    installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.GG - May
    be any two digit combination of letters.  If blank, cover is black or if filled in
    indicates colored covers or special labels on the cover.
[8] V2HABC-DD and V2HFABC-DD where:
    A  - May be D (downflow) or B (backwash only).
    B  - May be M (meter) or T (timer).
    C  - May be A, A2, A3, B, C, D, E, F, G, H or Z.  Indicates the injector installed.
    DD - May be any number from 01 to 99.  Indicates packaging or NPT or BSPT variations.
[9] Certified for use with tanks 18 x 65 and greater.
[G] Product is Certified to NSF/ANSI 372 and conforms with the lead content requirements for
    “lead free” plumbing as defined by California, Vermont, Maryland, and Louisiana state
    laws and the U.S. Safe Drinking Water Act.

    
[10] V3ABC-DD where:
     A  - May be D (downflow) or B (backwash only).
     B  - May be M (meter) or T (timer).
     C  - May be A, A2, A3, B, C, D, E, F, G, or H.  Indicates the injector installed.
     DD - May be any number from 01 to 99.  Indicates packaging or NPT or BSPT variations.
[11] V3006-XX where XX may be 01, 02 or 04.  Indicates handle color, handle direction or
     packaging.
[12] Certified for use with tanks 13 x 54 and greater.

	
Tanks[G] 

	10 X 13
	3.25 gal.
	CLD 23
	MLTPL
	

	10 X 18
	4.75 gal.
	CLD 23
	MLTPL
	

	10 X 35
	10.24 gal.
	CLD 23
	MLTPL
	

	10 X 40
	12.02 gal.
	CLD 23
	MLTPL
	

	10 X 40 BTM PLT
	12.02 gal.
	CLD 23
	MLTPL
	

	10 X 44
	13.23 gal.
	CLD 23
	MLTPL
	

	10 X 44 BTM PLT
	13.23 gal.
	CLD 23
	MLTPL
	

	10 X 47
	14.2 gal.
	CLD 23
	MLTPL
	

	10 X 54
	16.02 gal.
	CLD 23
	MLTPL
	

	10 X 54 BTM & MID PLT
	16.01 gal.
	CLD 23
	MLTPL
	

	10 X 54 BTM PLT
	16.01 gal
	CLD 23
	MLTPL
	

	10 X 54 DH BTM PLT
	16.01 gal.
	CLD 23
	MLTPL
	

	10 X 54 DH MID & BTM PLT
	16.01 gal.
	CLD 23
	MLTPL
	

	10 X 54 DOME HOLE
	16.01 gal.
	CLD 23
	MLTPL
	

	12 X 35
	14.6 gal.
	CLD 23
	MLTPL
	

	12 X 48
	20.8 gal.
	CLD 23
	MLTPL
	

	12 X 52
	22.88 gal.
	CLD 23
	MLTPL
	

	12 X 52 BTM & MID PLT
	22.88 gal.
	CLD 23
	MLTPL
	

	12 X 52 BTM PLT
	22.88 gal.
	CLD 23
	MLTPL
	

	12 X 52 DH BTM PLT
	22.88 gal.
	CLD 23
	MLTPL
	

	12 X 52 DH MID & BTM PLT
	22.88 gal.
	CLD 23
	MLTPL
	

	12 X 52 DOME HOLE
	22.88 gal.
	CLD 23
	MLTPL
	

	13 X 54
	27.84 gal.
	CLD 23
	MLTPL
	

	13 X 54 BTM & MID PLT
	27.84 gal.
	CLD 23
	MLTPL
	

	13 X 54 BTM PLT
	27.84 gal.
	CLD 23
	MLTPL
	

	13 X 54 DH BTM PLT
	27.84 gal.
	CLD 23
	MLTPL
	

	13 X 54 DH MID & BTM PLT
	27.84 gal.
	CLD 23
	MLTPL
	

	13 X 54 DOME HOLE
	27.84 gal.
	CLD 23
	MLTPL
	

	14 x 65
	39.44 gal.
	CLD 23
	MLTPL
	

	16 x 53
	41.0 gal.
	CLD 23
	MLTPL
	

	16 x 65
	51.2 gal.
	CLD 23
	MLTPL
	

	18 x 65
	73.48 gal.
	CLD 23
	MLTPL
	

	21 x 62
	89.59 gal.
	CLD 23
	MLTPL
	

	24 x 72
	122.61 gal.
	CLD 23
	MLTPL
	

	30 X 72
	193.48 gal.
	CLD 23
	MLTPL
	

	35 X 72
	277.71 gal.
	CLD 23
	MLTPL
	

	8 X 35
	6.73 gal.
	CLD 23
	MLTPL
	

	8 X 44
	8.59 gal.
	CLD 23
	MLTPL
	

	9 X 18
	3.92 gal.
	CLD 23
	MLTPL
	

	9 X 35
	8.19 gal.
	CLD 23
	MLTPL
	

	9 X 44 BTM PLT
	10.50 gal.
	CLD 23
	MLTPL
	

	9 X 48
	11.53 gal.
	CLD 23
	MLTPL
	

	9 X 48 BTM PLT
	11.53 gal.
	CLD 23
	MLTPL
	

	MCT120-C2253
	120 gal.
	CLD 23
	MLTPL
	

	RT120-C2252
	120 gal.
	CLD 23
	MLTPL
	

	RT40-C2250
	40 gal.
	CLD 23
	MLTPL
	

	RT80-C2251
	80 gal.
	CLD 23
	MLTPL
	

	
[G] Product is Certified to NSF/ANSI 372 and conforms with the lead content requirements for
    “lead free” plumbing as defined by California, Vermont, Maryland, and Louisiana state
    laws and the U.S. Safe Drinking Water Act.

    



Process Media

	 
	 
	Water
	Water

	 
	 
	Contact
	Contact

	Trade Designation
	Size
	Temp
	Material

	
Oxidative Media [G] 

	Birm®[1]
	12x50 mesh
	CLD 23
	MNDOX
	

	
[1] Certified for a minimum flow rate of 3.5 gpm/sq. ft (142 lpm/sq. m), using a bed depth
    of 30-36 in (76-91 cm).
[G] Product is Certified to NSF/ANSI 372 and conforms with the lead content requirements for
    “lead free” plumbing as defined by California, Vermont, Maryland, and Louisiana state
    laws and the U.S. Safe Drinking Water Act.

    



NOTE: Certified for water treatment plant applications.
      This product has not been evaluated for point of use applications.

