NSF/ANSI 44
Cation Exchange Water Softeners
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Facility : Windsor, WI
	 
	 
	 
	 
	 
	 
	 

	
COMPONENTS: Fittings[1] [Pb] [POE] 

	3/4" Brass Sweat Assembly LF - V3007-03LF[2]
	
	 
	 
	 
	 
	

	3/4" John Guest QC Elbow Assembly - V3007-15[2]
	
	 
	 
	 
	 
	

	3/4" John Guest QC Straight Assembly - V3007-19[2]
	
	 
	 
	 
	 
	

	3/4" Plastic Male BSPT Assembly - V3007-14[2]
	
	 
	 
	 
	 
	

	3/4" Plastic Male NPT Assembly - V3007-18[2]
	
	 
	 
	 
	 
	

	3/4" Sharkbite® Assembly - V3007-12LF[2]
	
	 
	 
	 
	 
	

	3/4" x 1" PVC Solvent Elbow Assembly - V3007-01[2]
	
	 
	 
	 
	 
	

	1" Brass Sweat Assembly LF - V3007-02LF[2]
	
	 
	 
	 
	 
	

	1" John Guest QC Elbow Assembly - V3007-20[2]
	
	 
	 
	 
	 
	

	1" John Guest Straight QC Assembly - V3007-17[2]
	
	 
	 
	 
	 
	

	1" Meter Assembly - V3039[2]
	
	 
	 
	 
	 
	

	1" Meter Assembly - V3039-15[2]
	
	 
	 
	 
	 
	

	1" Plastic Male BSPT Assembly - V3007-06[2]
	
	 
	 
	 
	 
	

	1" Plastic Male NPT Assembly - V3007-04[2]
	
	 
	 
	 
	 
	

	1" PVC Male BSPT Elbow Assembly - V3007-16[2]
	
	 
	 
	 
	 
	

	1" PVC Male NPT Elbow Assembly - V3007[2]
	
	 
	 
	 
	 
	

	1" Sharkbite® Assembly - V3007-13LF[2]
	
	 
	 
	 
	 
	

	1.25" Plastic Male BSPT Assembly - V3007-08[2]
	
	 
	 
	 
	 
	

	1.25" Plastic Male NPT Assembly - V3007-05[2]
	
	 
	 
	 
	 
	

	1.25" & 1.5" Brass Sweat Assembly LF - V3007-09LF[2]
	
	 
	 
	 
	 
	

	1.25" & 1.5" PVC Solvent Assembly - V3007-07[2]
	
	 
	 
	 
	 
	

	Inline Vertical Adapter Fitting - V3467[2]
	
	 
	 
	 
	 
	

	Vertical Adapter Assembly - V3191-01[2]
	
	 
	 
	 
	 
	

	
   
[1] Conforms to material and structural integrity requirements.
[2] Certified for use with tanks 9 x 48 and greater.
[Pb] Product also evaluated and determined to possess weighted average lead content of
     <=0.25% and complies with lead content requirements for “lead free” plumbing as defined
     by California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking
     Water Act.
[POE] Product conforms to NSF/ANSI/CAN 61 health effects requirements.
	

	
COMPONENTS: Tanks, Water Softener[1] [Pb] [POE] 

	8 x 35
	
	 
	 
	 
	 
	

	8 x 44
	
	 
	 
	 
	 
	

	9 x 18
	
	 
	 
	 
	 
	

	9 x 35
	
	 
	 
	 
	 
	

	9 x 44 BTM PLT
	
	 
	 
	 
	 
	

	9 x 48
	
	 
	 
	 
	 
	

	9 x 48 BTM PLT
	
	 
	 
	 
	 
	

	10 X 13
	
	 
	 
	 
	 
	

	10 x 18
	
	 
	 
	 
	 
	

	10 x 35
	
	 
	 
	 
	 
	

	10 x 40
	
	 
	 
	 
	 
	

	10 x 40 BTM PLT
	
	 
	 
	 
	 
	

	10 x 44
	
	 
	 
	 
	 
	

	10 x 44 BTM PLT
	
	 
	 
	 
	 
	

	10 x 47
	
	 
	 
	 
	 
	

	10 x 54
	
	 
	 
	 
	 
	

	10 x 54 BTM & MID PLT
	
	 
	 
	 
	 
	

	10 x 54 BTM PLT
	
	 
	 
	 
	 
	

	10 x 54 DH BTM PLT
	
	 
	 
	 
	 
	

	10 x 54 DH MID & BTM PLT
	
	 
	 
	 
	 
	

	10 x 54 DOME HOLE
	
	 
	 
	 
	 
	

	12 x 35
	
	 
	 
	 
	 
	

	12 x 52
	
	 
	 
	 
	 
	

	12 x 52 BTM & MID PLT
	
	 
	 
	 
	 
	

	12 x 52 BTM PLT
	
	 
	 
	 
	 
	

	12 x 52 DH BTM PLT
	
	 
	 
	 
	 
	

	12 x 52 DH MID & BTM PLT
	
	 
	 
	 
	 
	

	12 x 52 DOME HOLE
	
	 
	 
	 
	 
	

	13 x 54
	
	 
	 
	 
	 
	

	13 x 54 BTM & MID PLT
	
	 
	 
	 
	 
	

	13 x 54 BTM PLT
	
	 
	 
	 
	 
	

	13 x 54 DH BTM PLT
	
	 
	 
	 
	 
	

	13 x 54 DH MID & BTM PLT
	
	 
	 
	 
	 
	

	13 x 54 DOME HOLE
	
	 
	 
	 
	 
	

	14 x 65
	
	 
	 
	 
	 
	

	16 x 53
	
	 
	 
	 
	 
	

	16 x 65
	
	 
	 
	 
	 
	

	18 x 65
	
	 
	 
	 
	 
	

	21 x 62
	
	 
	 
	 
	 
	

	24 x 72
	
	 
	 
	 
	 
	

	30 x 72
	
	 
	 
	 
	 
	

	35 x 72
	
	 
	 
	 
	 
	

	MCT120-C2253
	
	 
	 
	 
	 
	

	RT40-C2250
	
	 
	 
	 
	 
	

	RT80-C2251
	
	 
	 
	 
	 
	

	RT120-C2252
	
	 
	 
	 
	 
	

	
   
[1] Conforms to material and structural integrity requirements.
[Pb] Product also evaluated and determined to possess weighted average lead content of
     <=0.25% and complies with lead content requirements for “lead free” plumbing as defined
     by California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking
     Water Act.
[POE] Product conforms to NSF/ANSI/CAN 61 health effects requirements.
	

	
COMPONENTS: Tubing[3] [Pb] [POE] 

	DPMT-0948
	
	 
	 
	 
	 
	

	DPMT-0948-A
	
	 
	 
	 
	 
	

	DPMT-1054
	
	 
	 
	 
	 
	

	DPMT-1054-A
	
	 
	 
	 
	 
	

	DPMT-1054-32MM 
	
	 
	 
	 
	 
	

	DPMT-1054-1320
	
	 
	 
	 
	 
	

	DPMT-1252
	
	 
	 
	 
	 
	

	DPMT-1252-A
	
	 
	 
	 
	 
	

	DPMT-1252-32MM
	
	 
	 
	 
	 
	

	DPMT-1252-1320
	
	 
	 
	 
	 
	

	DPMT-1354
	
	 
	 
	 
	 
	

	DPMT-1354-32MM
	
	 
	 
	 
	 
	

	DPMT-1354-1320 
	
	 
	 
	 
	 
	

	DPMT-1354-A
	
	 
	 
	 
	 
	

	
   
[3] Certified for use with tanks 10 x 54 and greater.
[Pb] Product also evaluated and determined to possess weighted average lead content of
     <=0.25% and complies with lead content requirements for “lead free” plumbing as defined
     by California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking
     Water Act.
[POE] Product conforms to NSF/ANSI/CAN 61 health effects requirements.
	

	
COMPONENTS: Valves, Diverter, Point-of-Entry[1] [Pb] [POE] 

	1" Bypass Assembly - V3006[2]
	
	 
	 
	 
	 
	

	1" Bypass Assembly - V3006-XX[2] [5]
	
	 
	 
	 
	 
	

	1" Control Valve - WS1XX - V1AABCD-EFFGG[2] [4]
	
	 
	 
	 
	 
	

	1" Twin Control Valve - TT1XX - VTT1AABCD-EFFGG[2] [4]
	
	 
	 
	 
	 
	

	1" & 1.25" Motorized Alternating Valve - V3069MM-01[2]
	
	 
	 
	 
	 
	

	1" & 1.25" Motorized Alternating Valve - V3069FF-01[2]
	
	 
	 
	 
	 
	

	1" & 1.25" No Hard Water Bypass Valve - V3070FM[2]
	
	 
	 
	 
	 
	

	1" & 1.25" No Hard Water Bypass Valve - V3070FF[2]
	
	 
	 
	 
	 
	

	1.25" Control Valve - WS125XX - V125AABCD-EFFGG[2] [4]
	
	 
	 
	 
	 
	

	1191 In-Out Head - D1400[2]
	
	 
	 
	 
	 
	

	1191 In-Out Head w/ 1.320in Riser - D1400-03[2]
	
	 
	 
	 
	 
	

	1190FP In-Out Head w/ Fill Port - D1220-01[2]
	
	 
	 
	 
	 
	

	External In-Line Mixing Valve - V4099[2]
	
	 
	 
	 
	 
	

	
   
[1] Conforms to material and structural integrity requirements.
[2] Certified for use with tanks 9 x 48 and greater.
[4] V1AABCD-EFFGG, VTT1AABCD-EFFGG and V125AABCD-EFFGG where:
    AA - May be blank or any two digit letter code
    B  - May be D (downflow, U (upflow), or B (backwash only)
    C  - May be M (meter) or T (timer)
    D  - May be A, A2, A3, B, C, D, E, F, G, H, I, J, K, or Z to indicate the injector 
         installed
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve
    FF - May be any number from 01 to 99.  Indicates packaging or base variations
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    
         in indicates colored covers or special labels on the cover.
[5] V3006-XX where XX may be 01, 02 or 04.  Indicates handle color, handle direction or
    packaging.
[Pb] Product also evaluated and determined to possess weighted average lead content of
     <=0.25% and complies with lead content requirements for “lead free” plumbing as defined
     by California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking
     Water Act.
[POE] Product conforms to NSF/ANSI/CAN 61 health effects requirements.
	



