PART 1
NSF/ANSI/CAN 372 
Drinking Water System Components - Lead Content 



 
	Clack Corporation 
	

	4462 Duraform Lane
	

	Windsor, WI 53598-9716
	
	 

	United States
	
	 

	608-846-3010
	
	



Facility : Windsor, WI
	
Miscellaneous Treatment Devices/Components [LL] 

	   1" & 1.25" Motorized Alternating Valve - V3069FF-01



	   1" & 1.25" Motorized Alternating Valve - V3069MM-01



	   1" & 1.25" No Hard Water Bypass Valve - V3070FF



	   1" & 1.25" No Hard Water Bypass Valve - V3070FM



	   1" Brass Sweat Assembly LF - V3007-02LF



	   1" Bypass Assembly - V3006



	   1" Bypass Assembly - V3006-XX[7]



	   1" Control Valve - WS1XX - V1AABCD-EFFGG[1]



	   1" John Guest QC Elbow Assembly - V3007-20[2]



	   1" John Guest Straight QC Assembly - V3007-17



	   1" Meter Assembly - V3039



	   1" Meter Assembly - V3039-15



	   1" PVC Male BSPT Elbow Assembly - V3007-16



	   1" PVC Male NPT Elbow Assembly - V3007



	   1" Plastic Male BSPT Assembly - V3007-06



	   1" Plastic Male NPT Assembly - V3007-04



	   1" Sharkbite® Assembly - V3007-13LF



	   1" Twin Control Valve - TT1XX - VTT1AABCD-EFFGG[1]



	   1.25" Brass Sweat Assembly LF - V3007-09LF



	   1.25" Control Valve - WS125XX - V125AABCD-EFFGG[1]



	   1.25" PVC Solvent Assembly - V3007-07



	   1.25" Plastic Male BSPT Assembly - V3007-08



	   1.25" Plastic Male NPT Assembly - V3007-05



	   1.5" BSPT Meter - V3040BSPT



	   1.5" BSPT Meter - V3040BSPT-15



	   1.5" BSPT Motorized Alternating Valve (MAV) - V3071BSPT



	   1.5" BSPT No Hard Water Bypass Valve (NHWBP) - V3097BSPT



	   1.5" Brass Sweat Assembly LF - V3007-09LF



	   1.5" Bypass Assembly - V4678[3]



	   1.5" Control Valve - WS15XX - V15AABCD-EFFGG[2]



	   1.5" NPT Meter - V3040



	   1.5" NPT Meter - V3040-15



	   1.5" NPT Motorized Alternating Valve (MAV) - V3071



	   1.5" NPT No Hard Water Bypass Valve (NHWBP) - V3097



	   1.5" PLASTIC FTG ASY QC TO NPT SS - V4430-11



	   1.5" PVC Solvent Assembly - V3007-07



	   1.5" Plastic Control Valve - WS15P XX - VP15AABCD-EFFGG[2] [3]



	   1.5" Plastic FTG ASY QC TO BSPT - V4430-02[3]



	   1.5" Plastic FTG ASY QC TO NPT - V4430-01[3]



	   1.5" Plastic FTG ASY QC TO QC - V4430-03[3]



	   1.5" Plastic FTG ASY QC to BSPT Elbow - V4430-08



	   1.5" Plastic FTG ASY QC to NPT Elbow - V4430-07



	   1.5" Plastic FTG ASY QC to QC Elbow - V4430-09



	   1.5" Plastic FTG ASY QC to Solvent - 4430-13[3]



	   1.5" Plastic METER ASY BSPT 15FT - V3045BSPT-15[3]



	   1.5" Plastic METER ASY BSPT 28IN - V3045BSPT[3]



	   1.5" Plastic METER ASY NPT 15FT - V3045-15[3]



	   1.5" Plastic METER ASY NPT 28IN - V3045[3]



	   1.5" Plastic METER ASY QC TO QC 15FT - V3045QC-15[3]



	   1.5" Plastic METER ASY QC TO QC 28IN - V3045QC[3]



	   1.5" Plastic Motorized Alternating Valve (MAV) - V3034[3]



	   1.5" Plastic No Hard Water Bypass Valve (NHWBP) - V3035[3]



	   1.5' PLASTIC FTG ASY QC TO BSPT SS - V4430-12



	   1190FP In-Out Head w/ Fill Port - D1220-01



	   1191 In-Out Head - D1400



	   1191 In-Out Head w/ 1.320in Riser - D1400-03



	   1192 1.5 IN/OUT HEAD - D1403



	   1192 50MM IN/OUT HEAD - D1403-01



	   2" BSPT Meter - V3094BSPT



	   2" BSPT Meter - V3094BSPT-15



	   2" BSPT Motorized Alternating Valve (MAV) - V3076BSPT



	   2" BSPT No Hard Water Bypass Valve (NHWBP) - V3098BSPT



	   2" Control Valve - WS2XX - V2AABCD-EFFGG[4]



	   2" HF Control Valve - WS2HF - V2HFABC-DD [5]



	   2" NPT Meter - V3094



	   2" NPT Meter - V3094-15



	   2" NPT Motorized Alternating Valve (MAV) - V3076



	   2" NPT No Hard Water Bypass Valve (NHWBP) - V3098



	   2" PLASTIC FTG ASY QC TO BSPT SS - V4460-12[9]



	   2" PLASTIC FTG ASY QC TO NPT SS - V4460-11[9]



	   2" Plastic Control Valve - WS2P XX - VP2AABCD-EFFGG[4]



	   2" Plastic FTG ASY QC TO BSPT - V4460-02[9]



	   2" Plastic FTG ASY QC TO NPT - V4460-01[9]



	   2" Plastic FTG ASY QC TO QC - V4460-03[9]



	   2" Plastic FTG ASY QC to BSPT Elbow - V4460-05[9]



	   2" Plastic FTG ASY QC to NPT Elbow - V4460-04[9]



	   2" Plastic FTG ASY QC to QC Elbow - V4460-06[9]



	   2" Plastic FTG ASY QC to Solvent - V4460-13[9]



	   2" Plastic METER ASY BSPT 15FT - V3048BSPT-15[9]



	   2" Plastic METER ASY BSPT 28IN - V3048BSPT[9]



	   2" Plastic METER ASY NPT 15FT - V3048-15[9]



	   2" Plastic METER ASY NPT 28IN - V3048[9]



	   2" Plastic METER ASY QC TO QC 15FT - V3048QC-15



	   2" Plastic METER ASY QC TO QC 28IN - V3048QC



	   2" Plastic Motorized Alternating Valve (MAV) - V3036



	   2" Plastic No Hard Water Bypass Valve (NHWBP) - V3037



	   2" Quick Connect Control Valve - WS2XX - V2AABCD-EFFGG[2]



	   2H Control Valve - WS2H - V2HABC-DD[5]



	   2” QC & 2H 4" BASE Assembly - V3064



	   2” QC & 2H 6" FLANGE BASE Assembly - V3055



	   2” QC & 2H BSPT SIDE MOUNT Assembly - V3260BSPT-02



	   2” QC & 2H NPT SIDE MOUNT Assembly - V3260-02



	   3" BSPT Meter - V3095BSPT



	   3" BSPT Meter - V3095BSPT-15



	   3" BSPT Motorized Alternating Valve (MAV) - V3083BSPT



	   3" BSPT No Hard Water Bypass Valve (NHWBP) - V3099BSPT



	   3" BSPT Side Mount Base Assembly - V3674-BSPT-02



	   3" Control Valve - WS3 -V3ABC-DD[6]



	   3" NPT Meter - V3095



	   3" NPT Meter - V3095-15



	   3" NPT Motorized Alternating Valve (MAV) - V3083



	   3" NPT No Hard Water Bypass Valve (NHWBP) - V3099



	   3" NPT Side Mount Base Assembly - V3674-02



	   3/4" Brass Sweat Assembly LF - V3007-03LF



	   3/4" John Guest QC Elbow Assembly - V3007-15



	   3/4" John Guest QC Straight Assembly - V3007-19



	   3/4" Plastic Male BSPT Assembly - V3007-14



	   3/4" Plastic Male NPT Assembly - V3007-18



	   3/4" Sharkbite® Assembly - V3007-12LF



	   3/4" x 1" PVC Solvent Elbow Assembly - V3007-01



	   6" Flange Base Assembly - V3090



	   Air Blocker - D1047



	   DPMT-0948



	   DPMT-0948-A



	   DPMT-1054[3]



	   DPMT-1054-1320[3]



	   DPMT-1054-32MM[3]



	   DPMT-1054-A



	   DPMT-1252



	   DPMT-1252-1320



	   DPMT-1252-32MM



	   DPMT-1252-A



	   DPMT-1354[8]



	   DPMT-1354-1320[8]



	   DPMT-1354-32MM[8]



	   DPMT-1354-A



	   External In-Line Mixing Valve - V4099



	   Inline Adapter Fitting - V3467



	   Vertical Adapter Assembly - V3191-01

	
[1] V1AABCD-EFFGG, VTT1AABCD-EFFGG, and V125AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be A, A2, A3, B, C, D, E, F, G, H, I, J, K, or Z to indicate the injector
    installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    in indicates colored covers or special labels on the cover.
[2] V15AABCD-EFFGG and VP15AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be B, C, D, E, F, G, H, I, or Z to indicate the injector installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    in indicates colored covers or special labels on the cover.
[3] Certified for use with tanks 10 x 54 and greater.
[4] V2AABCD-EFFGG and VP2AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be A, A2, A3, B, C, D, E, F, G, R, S, T, U, or Z to indicate the injector
    installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.GG - May
    be any two digit combination of letters.  If blank, cover is black or if filled in
    indicates colored covers or special labels on the cover.
[5] V2HABC-DD and V2HFABC-DD where:
    A  - May be D (downflow) or B (backwash only).
    B  - May be M (meter) or T (timer).
    C  - May be A, A2, A3, B, C, D, E, F, G, H or Z.  Indicates the injector installed.
    DD - May be any number from 01 to 99.  Indicates packaging or NPT or BSPT variations.
[6] V3ABC-DD where:
    A  - May be D (downflow) or B (backwash only).
    B  - May be M (meter) or T (timer).
    C  - May be A, A2, A3, B, C, D, E, F, G, or H.  Indicates the injector installed.
    DD - May be any number from 01 to 99.  Indicates packaging or NPT or BSPT variations.
    
    
[7] V3006-XX where XX may be 01, 02 or 04.  Indicates handle color, handle direction or
    packaging.
[8] Certified for use with tanks 13 x 54 and greater.
[9] Certified for use with tanks 12 x 52 and greater.
[LL] Product conforms with lead content requirements for “lead free” plumbing as defined by
     California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking Water
     Act.



	
Tanks[LL] 

	   10 X 13



	   10 x 18



	   10 x 35



	   10 x 40



	   10 x 40 BTM PLT



	   10 x 44



	   10 x 44 BTM PLT



	   10 x 47



	   10 x 54



	   10 x 54 BTM & MID PLT



	   10 x 54 BTM PLT



	   10 x 54 DH BTM PLT



	   10 x 54 DH MID & BTM PLT



	   10 x 54 DOME HOLE



	   12 x 35



	   12 x 48



	   12 x 52



	   12 x 52 BTM & MID PLT



	   12 x 52 BTM PLT



	   12 x 52 DH BTM PLT



	   12 x 52 DH MID & BTM PLT



	   12 x 52 DOME HOLE



	   13 x 54



	   13 x 54 BTM & MID PLT



	   13 x 54 BTM & MID PLT



	   13 x 54 BTM PLT



	   13 x 54 DH BTM PLT



	   13 x 54 DH MID & BTM PLT



	   13 x 54 DOME HOLE



	   14 x 65



	   16 x 53



	   16 x 65



	   18 x 65



	   21 x 62



	   24 x 72



	   30 x 72



	   35 x 72



	   8 x 35



	   8 x 44



	   9 x 18



	   9 x 35



	   9 x 44 BTM PLT



	   9 x 48



	   9 x 48 BTM PLT



	   MCT120-C2253



	   RT120-C2252



	   RT40-C2250



	   RT80-C2251

	
[LL] Product conforms with lead content requirements for “lead free” plumbing as defined by
     California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking Water
     Act.




PART 2
NSF/ANSI/CAN 372 
Drinking Water System Components - Lead Content 



 
	Clack Corporation 
	
	

	4462 Duraform Lane
	
	

	Windsor, WI 53598-9716
	
	 

	United States
	
	 

	608-846-3010
	
	



Facility : Windsor, WI

 	
	
Miscellaneous Treatment Devices/Components [LL] 

	   1" & 1.25" Motorized Alternating Valve - V3069FF-01



	   1" & 1.25" Motorized Alternating Valve - V3069MM-01



	   1" & 1.25" No Hard Water Bypass Valve - V3070FF



	   1" & 1.25" No Hard Water Bypass Valve - V3070FM



	   1" Brass Sweat Assembly LF - V3007-02LF



	   1" Bypass Assembly - V3006



	   1" Bypass Assembly - V3006-XX[7]



	   1" Control Valve - WS1XX - V1AABCD-EFFGG[1]



	   1" John Guest QC Elbow Assembly - V3007-20[2]



	   1" John Guest Straight QC Assembly - V3007-17



	   1" Meter Assembly - V3039



	   1" Meter Assembly - V3039-15



	   1" PVC Male BSPT Elbow Assembly - V3007-16



	   1" PVC Male NPT Elbow Assembly - V3007



	   1" Plastic Male BSPT Assembly - V3007-06



	   1" Plastic Male NPT Assembly - V3007-04



	   1" Sharkbite® Assembly - V3007-13LF



	   1" Twin Control Valve - TT1XX - VTT1AABCD-EFFGG[1]



	   1.25" Brass Sweat Assembly LF - V3007-09LF



	   1.25" Control Valve - WS125XX - V125AABCD-EFFGG[1]



	   1.25" PVC Solvent Assembly - V3007-07



	   1.25" Plastic Male BSPT Assembly - V3007-08



	   1.25" Plastic Male NPT Assembly - V3007-05



	   1.5" BSPT Meter - V3040BSPT



	   1.5" BSPT Meter - V3040BSPT-15



	   1.5" BSPT Motorized Alternating Valve (MAV) - V3071BSPT



	   1.5" BSPT No Hard Water Bypass Valve (NHWBP) - V3097BSPT



	   1.5" Brass Sweat Assembly LF - V3007-09LF



	   1.5" Bypass Assembly - V4678[3]



	   1.5" Control Valve - WS15XX - V15AABCD-EFFGG[2]



	   1.5" NPT Meter - V3040



	   1.5" NPT Meter - V3040-15



	   1.5" NPT Motorized Alternating Valve (MAV) - V3071



	   1.5" NPT No Hard Water Bypass Valve (NHWBP) - V3097



	   1.5" PLASTIC FTG ASY QC TO NPT SS - V4430-11



	   1.5" PVC Solvent Assembly - V3007-07



	   1.5" Plastic Control Valve - WS15P XX - VP15AABCD-EFFGG[2] [3]



	   1.5" Plastic FTG ASY QC TO BSPT - V4430-02[3]



	   1.5" Plastic FTG ASY QC TO NPT - V4430-01[3]



	   1.5" Plastic FTG ASY QC TO QC - V4430-03[3]



	   1.5" Plastic FTG ASY QC to BSPT Elbow - V4430-08



	   1.5" Plastic FTG ASY QC to NPT Elbow - V4430-07



	   1.5" Plastic FTG ASY QC to QC Elbow - V4430-09



	   1.5" Plastic FTG ASY QC to Solvent - 4430-13[3]



	   1.5" Plastic METER ASY BSPT 15FT - V3045BSPT-15[3]



	   1.5" Plastic METER ASY BSPT 28IN - V3045BSPT[3]



	   1.5" Plastic METER ASY NPT 15FT - V3045-15[3]



	   1.5" Plastic METER ASY NPT 28IN - V3045[3]



	   1.5" Plastic METER ASY QC TO QC 15FT - V3045QC-15[3]



	   1.5" Plastic METER ASY QC TO QC 28IN - V3045QC[3]



	   1.5" Plastic Motorized Alternating Valve (MAV) - V3034[3]



	   1.5" Plastic No Hard Water Bypass Valve (NHWBP) - V3035[3]



	   1.5' PLASTIC FTG ASY QC TO BSPT SS - V4430-12



	   1190FP In-Out Head w/ Fill Port - D1220-01



	   1191 In-Out Head - D1400



	   1191 In-Out Head w/ 1.320in Riser - D1400-03



	   1192 1.5 IN/OUT HEAD - D1403



	   1192 50MM IN/OUT HEAD - D1403-01



	   2" BSPT Meter - V3094BSPT



	   2" BSPT Meter - V3094BSPT-15



	   2" BSPT Motorized Alternating Valve (MAV) - V3076BSPT



	   2" BSPT No Hard Water Bypass Valve (NHWBP) - V3098BSPT



	   2" Control Valve - WS2XX - V2AABCD-EFFGG[4]



	   2" HF Control Valve - WS2HF - V2HFABC-DD [5]



	   2" NPT Meter - V3094



	   2" NPT Meter - V3094-15



	   2" NPT Motorized Alternating Valve (MAV) - V3076



	   2" NPT No Hard Water Bypass Valve (NHWBP) - V3098



	   2" PLASTIC FTG ASY QC TO BSPT SS - V4460-12[9]



	   2" PLASTIC FTG ASY QC TO NPT SS - V4460-11[9]



	   2" Plastic Control Valve - WS2P XX - VP2AABCD-EFFGG[4]



	   2" Plastic FTG ASY QC TO BSPT - V4460-02[9]



	   2" Plastic FTG ASY QC TO NPT - V4460-01[9]



	   2" Plastic FTG ASY QC TO QC - V4460-03[9]



	   2" Plastic FTG ASY QC to BSPT Elbow - V4460-05[9]



	   2" Plastic FTG ASY QC to NPT Elbow - V4460-04[9]



	   2" Plastic FTG ASY QC to QC Elbow - V4460-06[9]



	   2" Plastic FTG ASY QC to Solvent - V4460-13[9]



	   2" Plastic METER ASY BSPT 15FT - V3048BSPT-15[9]



	   2" Plastic METER ASY BSPT 28IN - V3048BSPT[9]



	   2" Plastic METER ASY NPT 15FT - V3048-15[9]



	   2" Plastic METER ASY NPT 28IN - V3048[9]



	   2" Plastic METER ASY QC TO QC 15FT - V3048QC-15



	   2" Plastic METER ASY QC TO QC 28IN - V3048QC



	   2" Plastic Motorized Alternating Valve (MAV) - V3036



	   2" Plastic No Hard Water Bypass Valve (NHWBP) - V3037



	   2" Quick Connect Control Valve - WS2XX - V2AABCD-EFFGG[2]



	   2H Control Valve - WS2H - V2HABC-DD[5]



	   2” QC & 2H 4" BASE Assembly - V3064



	   2” QC & 2H 6" FLANGE BASE Assembly - V3055



	   2” QC & 2H BSPT SIDE MOUNT Assembly - V3260BSPT-02



	   2” QC & 2H NPT SIDE MOUNT Assembly - V3260-02



	   3" BSPT Meter - V3095BSPT



	   3" BSPT Meter - V3095BSPT-15



	   3" BSPT Motorized Alternating Valve (MAV) - V3083BSPT



	   3" BSPT No Hard Water Bypass Valve (NHWBP) - V3099BSPT



	   3" BSPT Side Mount Base Assembly - V3674-BSPT-02



	   3" Control Valve - WS3 -V3ABC-DD[6]



	   3" NPT Meter - V3095



	   3" NPT Meter - V3095-15



	   3" NPT Motorized Alternating Valve (MAV) - V3083



	   3" NPT No Hard Water Bypass Valve (NHWBP) - V3099



	   3" NPT Side Mount Base Assembly - V3674-02



	   3/4" Brass Sweat Assembly LF - V3007-03LF



	   3/4" John Guest QC Elbow Assembly - V3007-15



	   3/4" John Guest QC Straight Assembly - V3007-19



	   3/4" Plastic Male BSPT Assembly - V3007-14



	   3/4" Plastic Male NPT Assembly - V3007-18



	   3/4" Sharkbite® Assembly - V3007-12LF



	   3/4" x 1" PVC Solvent Elbow Assembly - V3007-01



	   6" Flange Base Assembly - V3090



	   Air Blocker - D1047



	   DPMT-0948



	   DPMT-0948-A



	   DPMT-1054[3]



	   DPMT-1054-1320[3]



	   DPMT-1054-32MM[3]



	   DPMT-1054-A



	   DPMT-1252



	   DPMT-1252-1320



	   DPMT-1252-32MM



	   DPMT-1252-A



	   DPMT-1354[8]



	   DPMT-1354-1320[8]



	   DPMT-1354-32MM[8]



	   DPMT-1354-A



	   External In-Line Mixing Valve - V4099



	   Inline Adapter Fitting - V3467



	   Vertical Adapter Assembly - V3191-01

	
[1] V1AABCD-EFFGG, VTT1AABCD-EFFGG, and V125AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be A, A2, A3, B, C, D, E, F, G, H, I, J, K, or Z to indicate the injector
    installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    in indicates colored covers or special labels on the cover.
[2] V15AABCD-EFFGG and VP15AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be B, C, D, E, F, G, H, I, or Z to indicate the injector installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.
    GG - May be any two digit combination of letters.  If blank, cover is black or if filled
    in indicates colored covers or special labels on the cover.
[3] Certified for use with tanks 10 x 54 and greater.
[4] V2AABCD-EFFGG and VP2AABCD-EFFGG where:
    AA - May be blank or any two digit letter code.
    B  - May be D (downflow), U (upflow), or B (backwash only).
    C  - May be M (meter) or T (timer).
    D  - May be A, A2, A3, B, C, D, E, F, G, R, S, T, U, or Z to indicate the injector
    installed.
    E  - May be blank or any letter code.  If E or M then it includes a mixing valve.
    FF - May be any number from 01 to 99.  Indicates packaging or base variations.GG - May
    be any two digit combination of letters.  If blank, cover is black or if filled in
    indicates colored covers or special labels on the cover.
[5] V2HABC-DD and V2HFABC-DD where:
    A  - May be D (downflow) or B (backwash only).
    B  - May be M (meter) or T (timer).
    C  - May be A, A2, A3, B, C, D, E, F, G, H or Z.  Indicates the injector installed.
    DD - May be any number from 01 to 99.  Indicates packaging or NPT or BSPT variations.
[6] V3ABC-DD where:
    A  - May be D (downflow) or B (backwash only).
    B  - May be M (meter) or T (timer).
    C  - May be A, A2, A3, B, C, D, E, F, G, or H.  Indicates the injector installed.
    DD - May be any number from 01 to 99.  Indicates packaging or NPT or BSPT variations.
    
    
[7] V3006-XX where XX may be 01, 02 or 04.  Indicates handle color, handle direction or
    packaging.
[8] Certified for use with tanks 13 x 54 and greater.
[9] Certified for use with tanks 12 x 52 and greater.
[LL] Product conforms with lead content requirements for “lead free” plumbing as defined by
     California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking Water
     Act.




	
Tanks[LL] 

	   10 X 13



	   10 x 18



	   10 x 35



	   10 x 40



	   10 x 40 BTM PLT



	   10 x 44



	   10 x 44 BTM PLT



	   10 x 47



	   10 x 54



	   10 x 54 BTM & MID PLT



	   10 x 54 BTM PLT



	   10 x 54 DH BTM PLT



	   10 x 54 DH MID & BTM PLT



	   10 x 54 DOME HOLE



	   12 x 35



	   12 x 48



	   12 x 52



	   12 x 52 BTM & MID PLT



	   12 x 52 BTM PLT



	   12 x 52 DH BTM PLT



	   12 x 52 DH MID & BTM PLT



	   12 x 52 DOME HOLE



	   13 x 54



	   13 x 54 BTM & MID PLT



	   13 x 54 BTM & MID PLT



	   13 x 54 BTM PLT



	   13 x 54 DH BTM PLT



	   13 x 54 DH MID & BTM PLT



	   13 x 54 DOME HOLE



	   14 x 65



	   16 x 53



	   16 x 65



	   18 x 65



	   21 x 62



	   24 x 72



	   30 x 72



	   35 x 72



	   8 x 35



	   8 x 44



	   9 x 18



	   9 x 35



	   9 x 44 BTM PLT



	   9 x 48



	   9 x 48 BTM PLT



	   MCT120-C2253



	   RT120-C2252



	   RT40-C2250



	   RT80-C2251

	
[LL] Product conforms with lead content requirements for “lead free” plumbing as defined by
     California, Vermont, Maryland, and Louisiana state laws and the U.S. Safe Drinking Water
     Act.




